# Examples

Readme | IAR 5.x | GNU | Description
--- | --- | --- | ---
|  |  | Basic AC97 Project Plays and records sound through the on-board AC97 codec.
|  |  | Basic AES Project Uses the hardware AES to encrypt and decrypt test values in several operating modes.
|  |  | Basic Barometer Project Displays the current temperature and pressure using the on-board MS5540B sensor of the AT91SAM7L-EK.
|  |  | Basic Calculator Project Example of an application which uses the SAM7L backup modes.
|  |  | Basic CAN Project Demonstrates usage of the Controller Area Network (CAN) peripheral.
|  |  | Basic Dataflash Project Performs erase, read and write operations on the dataflash connected to the evaluation kit.
|  |  | Basic Dhrystone Project Computes the number of dhrystone per seconds that the chip can generate under different configurations.
|  |  | Basic EMAC Project Enables the device to respond to ICMP ECHO requests sent on the network.
|  |  | Basic EMAC lwIP Project Webserver example using the lwIP library.
|  |  | Basic EMAC µIP Project Webserver & telnet examples using the µIP library.
|  |  | Basic Internal Flash Project Performs several commands on the internal flash using the EFC.
|  |  | Basic ISO 7816 Project Sends ISO 7816 commands to a smartcard connected to the evaluation kits.
|  |  | Basic Keyboard Matrix Project Shows how to handle the keyboard matrix of the AT91SAM7L-EK.
|  |  | Basic LCD Project Displays images on the external on-board LCD screen.
|  |  | Basic Low Power Project Demonstrates the low power modes available on the SAM7L.
|  |  | Basic Low Power Project Demonstrates the low power modes available on the SAM7L.
|  |  | Basic NandFlash Project Erases and writes an external NandFlash memory chip.
|  |  | Basic NorFlash Project Erases and writes an external NorFlash memory chip.
|  |  | Basic PWM Project Makes one or more LEDs glow using a PWM signal.
|  |  | Basic RTC Project Demonstrates basic usage of the Real-Time Clock (RTC) peripheral.
|  |  | Basic RTT Project Demonstrates basic usage of the Real-Time Timer (RTT) peripheral.
|  |  | Basic SD Card Project Performs read & write tests on a SD card connected to the evaluation board.
|  |  | Basic Serial Flash Project Performs erase, read and write operations on an external Serial Firmware Dataflash chip connected to the board.
|  |  | Basic Segment LCD Project Displays information on the external on-board segment LCD.
|  |  | Basic Segment LCD Project Displays information on the external on-board segment LCD.
|  |  | Basic SSC-I2S AT73C213 Project Plays sound with the SSC in I2S mode, through an on-board AT73C213 DAC.
|  |  | Basic Triple-DES Project Uses the hardware triple-DES to encrypt and decrypt test values in several operating modes.
|  |  | Basic Touchscreen Project Enables the user to draw on the LCD with a stylus using the touchscreen.
|  |  | Basic TWI EEPROM Project Reads and writes an external TWI serial EEPROM.
|  |  | Basic USART Hardware Handshaking Project Regulates the speed of a USART file transfer using RTS/CTS hardware handshaking.
|  |  | SAM7L-EK Demo Project Demonstrations of several features of the AT91SAM7L-EK and the SAM7L family.
|  |  | LCD Slideshow Project Displays a slideshow animation on the LCD, made up from BMP images sent over a USB virtual COM port.

Please apply the IAR patch for softpack 1.4 provided by Atmel before using the IAR examples.

###### Atmel Corporation ©2008