#
# Device depenent key layout
# This example is for iPAQ h3100-h5500 series.
#

[Global]
image = /usr/share/pixmaps/ipaq-s1.png
offset_x = 50
offset_y = 10

[Power]
title = Power Button
symbol = gpe-config-apm.png
key = XF86PowerDown
modificator = ???Pressed
command = apm --suspend
xpos = 155
ypos = 0

[Record]
title = Audio Record
symbol = ibutton1.png
key = XF86Record
modificator = ???Pressed
command = gpe-soundbite record --autogenerate-filename $HOME_VOLATILE
xpos = 30
ypos = 30

[Calendar]
title = Calendar
symbol = ibutton2.png
key = XF86Calendar
modificator = ???Pressed
command = gpe-calendar
xpos = 57
ypos = 131

[Contacts]
title = Calendar
symbol = ibutton3.png
key = telephone
modificator = ???Pressed
command = gpe-contacts
xpos = 84
ypos = 143

[Mail]
title = Mail
symbol = ibutton4.png
key = XF86Mail
modificator = ???Pressed
command = gpe-taskmgr
xpos = 125
ypos = 144

[Start]
title = Calendar
symbol = ibutton5.png
key = XF86Start
modificator = ???Pressed
command = matchbox-remote -desktop
xpos = 168
ypos = 130
