##
## Each of these may be assigned to the number of nanoseconds by which to
## increase the timing of pcmcia bus transactions 
##
# COMPACTFLASH_TIMING_INCREMENT=0
## the single pcmcia sleeve seems to be a bit slow, but 25ns makes my
## orinoco card detectable. -Jamey 4/2/2002 
PCMCIA_TIMING_INCREMENT=25
# DUAL_PCMCIA_TIMING_INCREMENT=0

## mount options used by MMC
MMC_MOUNT_OPTIONS="-t auto -o sync,noatime"
